Minimoog wire colors

Keyboard Cinch-Jones	PL1

Keyboard					Moog
Male  (resistor color used)			Female		Other end connects to
1	Brown					Gray			
2	Red					White w/Brown	
3	Orange				White			
4	Yellow				Red			
5	Green					Green			
6	Blue					White w/Orange	

Modulation section Cinch-Jones PL2
						Other end connects to
1	Brown					SW1-3
2	Yellow				C03-1
3	Orange				C01A-4
4	Red					+10 volts
5	White					Ground
6	Blue (2)				C02A-7 and Glide pot tract (1)
7	Violet (2)				C02A-8 and Glide pot wiper (2)
8	White w/Gray			C02B-6
9	White w/Violet			C02B-15
10	White w/Blue (2)			C02B-2 and C02B-8
11	White w/Green			C02B-21
12	White w/Yellow			C02B-22